SOILTYPE_CLASSIF = zobler 
SOILALB_FILE     = soils_param.nc
SOILCLASS_FILE   = soils_param.nc

# DO_RSOIL : Reduce soil evaporation with a soil resistance
DO_RSOIL = n

# To make AVAN and NVAN constant with depth
CWRR_AKS_A0 = 0.
CWRR_AKS_POWER = 0.
CWRR_NKS_A0 = 0.
CWRR_NKS_POWER = 0.

#**************************************************************************

# STRESS_GS, STRESS_GM, STRESS_VCMAX : Stress on GS, GM and VCMAX (15 values, without space to have short line readable)
STRESS_GS=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.
STRESS_GM=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.
STRESS_VCMAX=1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.,1.

# Optimized parameters for albedo
ALB_LEAF_NIR = 0.,0.23,0.18,0.18,0.20,0.24,0.15,0.26,0.20,0.24,0.27,0.28,0.26
ALB_LEAF_VIS = 0.,0.04,0.04,0.04,0.04,0.03,0.03,0.03,0.03,0.06,0.06,0.06,0.06
SNOWA_AGED_NIR = 0.50,0,0,0.10,0.37,0.08,0.16,0.17,0.27,0.44,0.44,0.44,0.44
SNOWA_DEC_NIR = 0.13,0,0,0.10,0.10,0.16,0.04,0.07,0.08,0.12,0.12,0.12,0.12
SNOWA_AGED_VIS = 0.74,0,0,0.08,0.24,0.07,0.18,0.18,0.33,0.57,0.57,0.57,0.57
SNOWA_DEC_VIS = 0.21,0,0,0.14,0.08,0.17,0.05,0.06,0.09,0.15,0.15,0.15,0.15

# Optimized parameters for photosynthetic capacity 
VCMAX25__02 = 45.0
VCMAX25__03 = 45.0
VCMAX25__04 = 35.0
VCMAX25__05 = 40.0
VCMAX25__06 = 50.0
VCMAX25__07 = 45.0
VCMAX25__08 = 35.0
VCMAX25__09 = 35.0
VCMAX25__10 = 50.0
VCMAX25__11 = 50.0
VCMAX25__12 = 60.0
VCMAX25__13 = 60.0

# Optimized parameters for LAI
LAI_MAX__02 = 7.0
LAI_MAX__03 = 5.0
LAI_MAX__04 = 5.0
LAI_MAX__05 = 4.0
LAI_MAX__06 = 5.0
LAI_MAX__07 = 3.5
LAI_MAX__08 = 4.0
LAI_MAX__09 = 3.0
LAI_MAX__10 = 2.5
LAI_MAX__11 = 2.0
LAI_MAX__12 = 5.0
LAI_MAX__13 = 5.0

# Activate downregulation for CO2
DOWNREGULATION_CO2=y
DOWNREGULATION_CO2_BASELEVEL=380.

# Activate harvest of wood
DO_WOOD_HARVEST=n

# Growth respiration
FRAC_GROWTHRESP__02 = 0.35
FRAC_GROWTHRESP__03 = 0.35
FRAC_GROWTHRESP__04 = 0.28
FRAC_GROWTHRESP__05 = 0.28
FRAC_GROWTHRESP__06 = 0.28
FRAC_GROWTHRESP__07 = 0.35
FRAC_GROWTHRESP__08 = 0.35
FRAC_GROWTHRESP__09 = 0.35
FRAC_GROWTHRESP__10 = 0.28
FRAC_GROWTHRESP__11 = 0.28
FRAC_GROWTHRESP__12 = 0.28
FRAC_GROWTHRESP__13 = 0.28

# Maintenance respiration slope C
MAINT_RESP_SLOPE_C__02 = 0.12
MAINT_RESP_SLOPE_C__03 = 0.12
MAINT_RESP_SLOPE_C__04 = 0.16
MAINT_RESP_SLOPE_C__05 = 0.16
MAINT_RESP_SLOPE_C__06 = 0.16
MAINT_RESP_SLOPE_C__07 = 0.25
MAINT_RESP_SLOPE_C__08 = 0.25
MAINT_RESP_SLOPE_C__09 = 0.25
MAINT_RESP_SLOPE_C__10 = 0.16
MAINT_RESP_SLOPE_C__11 = 0.12
MAINT_RESP_SLOPE_C__12 = 0.16
MAINT_RESP_SLOPE_C__13 = 0.12

# Soil turnover
CARBON_TAU_ISLOW = 7
CARBON_TAU_IPASSIVE = 300

# Parameters related to surface and thermal physical properties
#************************************************************************
# Read bare soil albedo from file with background MODIS data
ALB_BG_MODIS = y
ALB_BG_FILE  = alb_bg.nc

# ROUGH_DYN : Account for a dynamic roughness height (activation of Su et al. parametrization)
ROUGH_DYN=y

# OK_FREEZE :  Activate the complet soil freezing scheme
OK_FREEZE=y

# DEPTH_MAX_T (m) :  Maximum depth of the soil thermodynamics
DEPTH_MAX_T=90

# OK_EXPLICITSNOW :  Activate explict snow scheme
OK_EXPLICITSNOW=y
 
# READ_REFTEMP :  Initialize soil temperature using climatological temperature
READ_REFTEMP=y

# Deactivate fire
FIRE_DISABLE=y
