# $HeadURL: svn://forge.ipsl.fr/orchidee/trunk/ORCHIDEE_OL/FG_CRUJRA_HIST/PARAM/run.def $
# $Date: 2023-05-12 13:04:57 +0200 (ven. 12 mai 2023) $
# $Revision: 8000 $
#
INCLUDEDEF=orchidee.def
INCLUDEDEF=orchidee_pft.def

# Parameters of the driver differ between the coupled and off-line configs
#**************************************************************************
# Time length for one intergration (default full lenght of forcing file)
START_DATE = _AUTO_
END_DATE = _AUTO_

# Time step of the SECHIBA component 
DT_SECHIBA = 1800

# Name of the forcing files read by the model
FORCING_FILE = forcing_yearm1.nc forcing_year.nc forcing_yearp1.nc

# Name of restart file for the driver (default NONE)
RESTART_FILEIN = _AUTOBLOCKER_

# Value for atmospheric CO2 could be interactive (LMDz), a time series or fixed
# (default=350)
ATM_CO2 = _AUTO_: DEFAULT = 350.

# Domain description 
#**************************************************************************
GRID_FILE = NONE

# Off-line configurations could be run for a smaller domain
# (default no limits are set, the full domain on the forcing file is used)
#**************************************************************************
#LIMIT_WEST=8
#LIMIT_NORTH=48
#LIMIT_SOUTH=46
#LIMIT_EAST=10


# Time period over which to distribute the precipitation 
#**************************************************************************
# In the driver files precipitation is the accumulated value over the
# time step of the driver file (e.g. 6 hours). In ORCHIDEE it needs to
# be decided whether over which time period (in seconds) this precip will come
# down. Short periods make rain storms, long periods make drizzel.
# If users would define SPREAD_PREC_SEC in run.def, it is recommended to use 3600
# If users do not define SPREAD_PREC_SEC in run.def, then it is equal to half of the forcing time step if the latter GE 3h, otherwise it is the same duration as the forcing time step



