\begin{equation}
\Delta B = B \times \frac{\Delta t} {tau_leaffall}
\end{equation}
where $B$ is the biomass, $\Delta B$ is the fraction of biomass lost, $\Delta t$ is the times step (1 day)
and $tau_leaffall$ is the time constant of meteorological determined turnover.
