\begin{equation}
gdd_{min} = \frac{603}{\exp(0.0091*NCD(i,j))} - 64. 
\end{equation}
where i and j are the grid cell and PFT, respectively. 
